**Pairing the RC-PR5 with SX**

**Setting up SX**

1. Power on SX and in main screen select **CONFIG**
2. Chose option number 5 – **COMMS**
3. In **COMMS SETUP** tab select **BLUETOOTH** as Comms mode
4. To save settings press OK in the same screen

**Setting up RC-PR5**

1. While SX powered on and running with settings mentioned earlier, power on RC-PR5 while holding **SEARCH** button down
2. As a result of a previous step **FAR led** will start to flash indicating searching for Bluetooth devices is in progress. **NOTE:** to speed up search process be sure there are almost zero visible Bluetooth devices in range.
3. Indication that RC-PR5 found SX is that COM LED1 and FAR led are both on continuously and on SX’s main screen you see total station icon with green antenna up
4. If previous statement is true then press FAR button to confirm pairing to SX. RC-PR5 powers off itself. Otherwise proceed with next step.
5. Press SEARCH button which will tell RC-PR5 to continue looking for next Bluetooth device. Continue search till on SX screen you see total station icon with green antenna up. Confirm pairing by pressing FAR button.